# Visual aspects of ZSP

Indoor unit has rounded edges and the lower front corner is strongly chamfered.
It is has glossy surface texture which is easy to keep clean
Soft and unstriking appearance

# Other
· This model is oriented towards cooling.
· Automatic drying mode after cooling can be enabled, dries internal wet surfaces with air circulation for 2 hours after unit has been shut down preventing mold and wet rag smell.
· Simplified remote controller for ease of use
· Indoor unit has humidity sensor, which prevents dew point formation on air conditioner surfaces during abnormal humidity levels
· Wifi is third party supplied option, like Combicontrol

#Image catalog

sisayksikko.jpg : ZSP indoor unit installed over the doorway in flat apartment
ulkoyksikko.jpg : ZSP outdoor unit installed into a balcony in flat apartment.
Zsp-kake.jpg: Picture of the remote controller of indoor unit
